baseschematic: ..\..\..\..\..\..\..\DVM -- PFC_CCM_sync_DLL.sxsch
log_file: ..\..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: LL_Nominal|F_Low|Disabled|100% Load|BodePlot
datetimestamp: 22/03/2022 07:01
status: RUN
scalar: Power(SRC)=103.47208
scalar: Power(LOAD)=100.04786
scalar: Efficiency=96.690688%
spec: Min_VLOAD=pass,Min. Output1 Voltage (397.79) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (402.42) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 11
graphid: 4237
graphname: Output#pop
sg: simplis_pop8_4237
path: simplis_pop8_4237.sxgph
graphid: 4248
graphname: Vdc-Vdrain#pop
sg: simplis_pop8_4248
path: simplis_pop8_4248.sxgph
graphid: 4264
graphname: SIGNAL#pop
sg: simplis_pop8_4264
path: simplis_pop8_4264.sxgph
graphid: 4275
graphname: Samples#pop
sg: simplis_pop8_4275
path: simplis_pop8_4275.sxgph
graphid: 4296
graphname: COMP#pop
sg: simplis_pop8_4296
path: simplis_pop8_4296.sxgph
graphid: 4317
graphname: triggers#pop
sg: simplis_pop8_4317
path: simplis_pop8_4317.sxgph
graphid: 4328
graphname: VL#pop
sg: simplis_pop8_4328
path: simplis_pop8_4328.sxgph
scalar: Min(VSRC)=-169.99978
scalar: Avg(VSRC)=-275.91442p
scalar: RMS(VSRC)=120.208
scalar: Pk2Pk(VSRC)=339.99957
scalar: Max(VSRC)=169.99978
scalar: Pk2Pk(ISRC)=2.4795665
scalar: Min(ISRC)=-1.2397832
scalar: RMS(ISRC)=861.02898m
scalar: Avg(ISRC)=-294.47158p
scalar: Max(ISRC)=1.2397832
graphid: 4339
graphname: DVM SRC#pop
sg: simplis_pop8_4339
path: simplis_pop8_4339.sxgph
curve4348:VSRC,FF0000
curve4362:ISRC,008000
png: simplis_pop8_4339.png
scalar: Min(VLOAD)=397.79008
scalar: Avg(VLOAD)=400.09244
scalar: RMS(VLOAD)=400.09572
scalar: Pk2Pk(VLOAD)=4.6295958
scalar: Max(VLOAD)=402.41968
scalar: Avg(ILOAD)=250.05778m
scalar: Max(ILOAD)=251.5123m
scalar: Pk2Pk(ILOAD)=2.8934974m
scalar: Min(ILOAD)=248.6188m
scalar: RMS(ILOAD)=250.05982m
graphid: 4350
graphname: DVM LOAD#pop
sg: simplis_pop8_4350
path: simplis_pop8_4350.sxgph
curve4359:VLOAD,FF0000
curve4365:ILOAD,008000
png: simplis_pop8_4350.png
graphid: 4382
graphname: Load_offset#pop
sg: simplis_pop8_4382
path: simplis_pop8_4382.sxgph
scalar: min_phase_freq=63.472646
scalar: min_phase=17.346815
scalar: phase_margin=58.866314
scalar: phase_crossover_freq=87.324127
scalar: gain_margin=28.991123
scalar: gain_crossover_freq=10.148314
graphid: 4438
graphname: DVM Bode Plot#ac
sg: simplis_ac55_4438
path: simplis_ac55_4438.sxgph
curve4447:PHASE,FF0000
curve4450:GAIN,008000
png: simplis_ac55_4438.png
spec: min_gain_margin=pass,Gain Margin (28.9911) is greater than Min. Gain Margin (12)
spec: min_phase_margin=pass,Phase Margin (58.8663) is greater than Min. Phase Margin (35)
rstatus: PASS
