baseschematic: ..\..\..\..\..\..\..\DVM -- PFC_CCM_sync_DLL.sxsch
log_file: ..\..\..\..\..\dvm_advanced.log
simulator: simplis
screenshot: schematic.png
deck: input.deck
init: input.deck.init
test_argument: LL_Nominal|F_Low|Disabled|80% Load|BodePlot
datetimestamp: 22/03/2022 07:37
status: RUN
scalar: Power(SRC)=82.986961
scalar: Power(LOAD)=80.038395
scalar: Efficiency=96.446953%
spec: Min_VLOAD=pass,Min. Output1 Voltage (398.243) is greater than or equal to Min. Output1 Voltage Spec (380)
spec: Max_VLOAD=pass,Max. Output1 Voltage (401.966) is less than or equal to Max. Output1 Voltage Spec (420)
stats: N/A
numgraphs: 11
graphid: 4753
graphname: Output#pop
sg: simplis_pop9_4753
path: simplis_pop9_4753.sxgph
graphid: 4764
graphname: Vdc-Vdrain#pop
sg: simplis_pop9_4764
path: simplis_pop9_4764.sxgph
graphid: 4780
graphname: SIGNAL#pop
sg: simplis_pop9_4780
path: simplis_pop9_4780.sxgph
graphid: 4791
graphname: Samples#pop
sg: simplis_pop9_4791
path: simplis_pop9_4791.sxgph
graphid: 4812
graphname: COMP#pop
sg: simplis_pop9_4812
path: simplis_pop9_4812.sxgph
graphid: 4833
graphname: triggers#pop
sg: simplis_pop9_4833
path: simplis_pop9_4833.sxgph
graphid: 4844
graphname: VL#pop
sg: simplis_pop9_4844
path: simplis_pop9_4844.sxgph
scalar: Min(VSRC)=-169.99978
scalar: Avg(VSRC)=-297.0842p
scalar: RMS(VSRC)=120.208
scalar: Pk2Pk(VSRC)=339.99957
scalar: Max(VSRC)=169.99978
scalar: Pk2Pk(ISRC)=1.9887787
scalar: Min(ISRC)=-994.38933m
scalar: RMS(ISRC)=690.74996m
scalar: Avg(ISRC)=-186.67489p
scalar: Max(ISRC)=994.38933m
graphid: 4855
graphname: DVM SRC#pop
sg: simplis_pop9_4855
path: simplis_pop9_4855.sxgph
curve4864:VSRC,FF0000
curve4878:ISRC,008000
png: simplis_pop9_4855.png
scalar: Max(VLOAD)=401.9655
scalar: Min(VLOAD)=398.24274
scalar: Avg(VLOAD)=400.09386
scalar: RMS(VLOAD)=400.09598
scalar: Pk2Pk(VLOAD)=3.7227638
scalar: Pk2Pk(ILOAD)=1.8613819m
scalar: Min(ILOAD)=199.12137m
scalar: RMS(ILOAD)=200.04799m
scalar: Avg(ILOAD)=200.04693m
scalar: Max(ILOAD)=200.98275m
graphid: 4866
graphname: DVM LOAD#pop
sg: simplis_pop9_4866
path: simplis_pop9_4866.sxgph
curve4875:VLOAD,FF0000
curve4881:ILOAD,008000
png: simplis_pop9_4866.png
graphid: 4898
graphname: Load_offset#pop
sg: simplis_pop9_4898
path: simplis_pop9_4898.sxgph
scalar: phase_margin=57.749992
scalar: phase_crossover_freq=88.372678
scalar: min_phase_freq=57.546639
scalar: min_phase=20.880963
scalar: gain_margin=29.384346
scalar: gain_crossover_freq=10.184492
graphid: 4954
graphname: DVM Bode Plot#ac
sg: simplis_ac56_4954
path: simplis_ac56_4954.sxgph
curve4963:PHASE,FF0000
curve4966:GAIN,008000
png: simplis_ac56_4954.png
spec: min_gain_margin=pass,Gain Margin (29.3843) is greater than Min. Gain Margin (12)
spec: min_phase_margin=pass,Phase Margin (57.75) is greater than Min. Phase Margin (35)
rstatus: PASS
